
1. Start an administrator command prompt by right-clicking

      Start -> All Programs -> Accessories -> Command Prompt

    and select "Run as Administrator".

2. In the administrator command prompt, execute the following command:

    regsvr32 “C:\Program Files (x86)\Jack\64bits\JackRouter.dll”
  
3. Start Jack.


You should now have an ASIO driver that sends and receives audio to and from jack.
In Radium, you can send and receive audio to and from these programs by
first creating "Jack Stereo In" and/or "Jack Stereo Out" audio objects in the Mixer,
and then routing sound the way you want it in the "Connections" window in
the qjackctl ("Jack Control") program.
